<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="34.29" y2="0" width="0" layer="20"/>
<wire x1="36.83" y1="2.54" x2="36.83" y2="22.225" width="0" layer="20"/>
<hole x="3.175" y="21.59" drill="3.2"/>
<hole x="33.655" y="21.59" drill="3.2"/>
<wire x1="0" y1="22.225" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="34.29" y1="24.765" x2="2.54" y2="24.765" width="0" layer="20"/>
<wire x1="34.29" y1="0" x2="36.83" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="36.83" y1="22.225" x2="34.29" y2="24.765" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="24.765" x2="0" y2="22.225" width="0" layer="20" curve="90"/>
<text>Base Station
v1.8</text>
<text>8</text>
<text>Base
Station
v1.8</text>
<text>1</text>
<text>1</text>
<text>2</text>
<text>1</text>
<text>2</text>
<text>G</text>
<text>5</text>
<text>G</text>
<text>5</text>
<text>5</text>
<text>G</text>
<text>5</text>
<text>G</text>
<text>1</text>
<text>2</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Andy-library">
<packages>
<package name="RJ45-8">
</package>
<package name="PLCC-2">
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="USB_HORZ_REINFORCED_MICRO">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="ftdichip">
<description>&lt;b&gt;FTDI (TM) CHIP&lt;/b&gt; Future Technology Devices International Ltd.&lt;p&gt;
http://www.ftdichip.com</description>
<packages>
<package name="SSOP16">
<description>&lt;b&gt;SSOP-16&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="Andy-library" package="RJ45-8" value="RJ45"/>
<element name="U2" library="SparkFun-DigitalIC" package="DIP08" value="TINY85-20-DIP">
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="IC1" library="ftdichip" package="SSOP16" value="FT230XS"/>
<element name="LED1" library="Andy-library" package="PLCC-2" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.1" value="100">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.1" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.1" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="AXIAL-0.1" value="27">
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="AXIAL-0.1" value="4.7k">
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="AXIAL-0.1" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="AXIAL-0.1" value="27">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100nF"/>
<element name="C6" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="4.7uF">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Andy-library" package="TO92-EBC-OVAL" value="2222A"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1" value="39">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="47pF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="47pF">
<attribute name="VALUE"/>
</element>
<element name="J1" library="Andy-library" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="PRT-00119"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="U$4" library="Andy-library" package="USB_HORZ_REINFORCED_MICRO" value="USB_SOCKET_MICRO_VERTREINFORCED"/>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="5"/>
<contactref element="U2" pad="4"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="5"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R15" pad="P$1"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="Q1" pad="E"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="GND"/>
<contactref element="U$4" pad="P5"/>
<contactref element="U$4" pad="G1"/>
<contactref element="U$4" pad="G2"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="OUT2">
<contactref element="U$3" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="R5" pad="P$1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="5VDC">
<contactref element="U$3" pad="4"/>
<contactref element="U2" pad="8"/>
<contactref element="IC1" pad="12"/>
<contactref element="LED1" pad="ANODE"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="12VDC">
<contactref element="U$3" pad="6"/>
</signal>
<signal name="3.3VDC">
<contactref element="U$3" pad="7"/>
</signal>
<signal name="IN2">
<contactref element="U$3" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="6"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="P$2"/>
<contactref element="Q1" pad="B"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="C"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="85_TX">
<contactref element="U2" pad="3"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="85_RX">
<contactref element="U2" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="OUT1">
<contactref element="U$3" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="R3" pad="P$1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="CATHODE"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="R14" pad="P$2"/>
<contactref element="U$4" pad="P1"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="3"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="15"/>
<contactref element="R14" pad="P$1"/>
<contactref element="R15" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="9"/>
<contactref element="R16" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="8"/>
<contactref element="R13" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="R16" pad="P$1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$4" pad="P2"/>
</signal>
<signal name="N$10">
<contactref element="R13" pad="P$2"/>
<contactref element="C2" pad="1"/>
<contactref element="U$4" pad="P3"/>
</signal>
<signal name="IN1">
<contactref element="U$3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
