<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="1.905" y1="0" x2="19.2405" y2="0" width="0" layer="20"/>
<wire x1="20.5105" y1="1.27" x2="20.5105" y2="15.24" width="0" layer="20"/>
<wire x1="0.635" y1="15.24" x2="0.635" y2="1.27" width="0" layer="20"/>
<wire x1="0.635" y1="1.27" x2="1.905" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.905" y1="16.51" x2="0.635" y2="15.24" width="0" layer="20" curve="90"/>
<wire x1="20.5105" y1="15.24" x2="19.2405" y2="16.51" width="0" layer="20" curve="90"/>
<wire x1="19.2405" y1="0" x2="20.5105" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="1.905" y1="16.51" x2="19.2405" y2="16.51" width="0" layer="20"/>
<text>Uploader 1.3</text>
</plain>
<libraries>
<library name="ftdichip">
<description>&lt;b&gt;FTDI (TM) CHIP&lt;/b&gt; Future Technology Devices International Ltd.&lt;p&gt;
http://www.ftdichip.com</description>
<packages>
<package name="SSOP16">
<description>&lt;b&gt;SSOP-16&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="Andy-library">
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="0805">
</package>
<package name="USB_HORZ_REINFORCED_MICRO">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="ftdichip" package="SSOP16" value="FT230XS">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="Andy-library" package="USB-A-H" value="USB-A-H"/>
<element name="C7" library="SparkFun-Passives" package="0805" value="47pF">
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0805" value="47pF">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="10nF">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0805" value="4.7uF">
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="R1" library="Andy-library" package="0805" value="27">
<attribute name="VALUE"/>
</element>
<element name="R2" library="Andy-library" package="0805" value="27">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="U$1" library="Andy-library" package="USB_HORZ_REINFORCED_MICRO" value="USB_SOCKET_MICRO_VERTREINFORCED"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP1" pad="GND3"/>
<contactref element="JP1" pad="GND2"/>
<contactref element="JP1" pad="GND"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U$1" pad="G2"/>
<contactref element="U$1" pad="G1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="5VDC">
<contactref element="IC1" pad="12"/>
<contactref element="JP1" pad="VBUS"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="84_TX">
<contactref element="IC1" pad="4"/>
<contactref element="U$1" pad="P1"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="3"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="9"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D+">
<contactref element="JP1" pad="D+"/>
<contactref element="C8" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="D-"/>
<contactref element="C7" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
