<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="24.765" y1="10.16" x2="1.905" y2="10.16" width="0" layer="20"/>
<wire x1="0" y1="8.255" x2="0" y2="1.905" width="0" layer="20"/>
<wire x1="1.905" y1="0" x2="24.765" y2="0" width="0" layer="20"/>
<wire x1="0" y1="8.255" x2="1.905" y2="10.16" width="0" layer="20" curve="-90"/>
<wire x1="24.765" y1="10.16" x2="26.67" y2="8.255" width="0" layer="20" curve="-90"/>
<wire x1="1.905" y1="0" x2="0" y2="1.905" width="0" layer="20" curve="-90"/>
<wire x1="26.67" y1="1.905" x2="24.765" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="26.67" y1="1.905" x2="26.67" y2="8.255" width="0" layer="20"/>
<text>Implant 4.4</text>
<text>POS</text>
<text>NEG</text>
</plain>
<libraries>
<library name="Andy-library">
<packages>
<package name="LASERDIODE">
</package>
<package name="0805">
</package>
<package name="USB_VERT_MICRO_SMD">
</package>
<package name="LED10MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Andy-library" package="LASERDIODE" value="LASERDIODE"/>
<element name="U$3" library="Andy-library" package="LASERDIODE" value="LASERDIODE"/>
<element name="R2" library="Andy-library" package="0805" value="6.8k">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02_SMALL" value="M02SMALL"/>
<element name="U$2" library="Andy-library" package="USB_VERT_MICRO_SMD" value="USB_SOCKET_MICRO_VERT"/>
<element name="LED1" library="Andy-library" package="LED10MM" value=""/>
</elements>
<signals>
<signal name="LD-">
<contactref element="U$3" pad="P$2"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$2" pad="P1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="LD+">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$2" pad="P5"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="P4"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="P2"/>
<contactref element="JP1" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="P$1"/>
<contactref element="R2" pad="2"/>
<contactref element="U$2" pad="P3"/>
</signal>
<signal name="HEATSINK">
<contactref element="U$1" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
